****

**Big 8 / Limited Latemodel**

We will follow the current Big 8 Series rules as they are written on the Big 8 web site: (<http://speedthrills.big8series.com/pdfs/12rules_01.pdf>), with the exceptions written below:

1. Weight: See separate weight rule.
2. The Lefthander ‘Quick Change Torque Link’, or similar device, is not allowed.
3. All ballast must be painted white, and have your car number painted on them. No piece of ballast may be less than 5 pounds. All ballast must be securely mounted to the frame or roll cage only. No ballast may be in the driver’s compartment.
4. All weights will be checked on the race track scales with the driver in the car.
5. Other engine combinations may be allowed WITH PRIOR APPROVAL from Tech Officials.